15.07.2019|19:03:40.995|[20]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): CoE - Emergency (Hex: %04x, %02x, '%02x %02x %02x %02x %02x').) (Drive 3 (CDHD)) (1002) (30082) (0) (0) (0) (0) (0) (0)
15.07.2019|19:03:41.014|[20]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): CoE - Emergency (Hex: %04x, %02x, '%02x %02x %02x %02x %02x').) (Drive 4 (CDHD)) (1003) (30082) (0) (0) (0) (0) (0) (0)
15.07.2019|19:03:41.027|[20]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): CoE - Emergency (Hex: %04x, %02x, '%02x %02x %02x %02x %02x').) (Drive 1 (CDHD)) (1001) (61568) (0) (0) (0) (0) (0) (0)
15.07.2019|19:03:41.061|[20]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): CoE - Emergency (Hex: %04x, %02x, '%02x %02x %02x %02x %02x').) (Drive 4 (CDHD)) (1003) (61568) (0) (0) (0) (0) (0) (0)
15.07.2019|19:03:41.075|[20]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): CoE - Emergency (Hex: %04x, %02x, '%02x %02x %02x %02x %02x').) (Drive 1 (CDHD)) (1001) (61568) (0) (0) (0) (0) (0) (0)
15.07.2019|19:03:41.109|[20]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): CoE - Emergency (Hex: %04x, %02x, '%02x %02x %02x %02x %02x').) (Drive 4 (CDHD)) (1003) (61568) (0) (0) (0) (0) (0) (0)
15.07.2019|19:03:41.123|[20]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): CoE - Emergency (Hex: %04x, %02x, '%02x %02x %02x %02x %02x').) (Drive 1 (CDHD)) (1001) (61568) (0) (0) (0) (0) (0) (0)
15.07.2019|19:03:41.157|[20]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): CoE - Emergency (Hex: %04x, %02x, '%02x %02x %02x %02x %02x').) (Drive 4 (CDHD)) (1003) (61568) (0) (0) (0) (0) (0) (0)
15.07.2019|19:04:24.013|[20]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): CoE - Emergency (Hex: %04x, %02x, '%02x %02x %02x %02x %02x').) (Drive 1 (CDHD)) (1001) (25472) (0) (0) (0) (0) (0) (0)
15.07.2019|19:04:24.021|[20]|ERROR|TcApplication.MainApp|Event (201), source (799) not found! (17056) (Group/axis consequential error) (Consequential error resulting from another causative error related to another axis within the group. Group/axis consequential errors can occur in relation to master/slave couplings or with multiple axis interpolating DXD groups. If, for instance, it is detected that the following error limit of a master axis has been exceeded, then this consequential error is assigned to all the other master axes and slave axes in this group.) (6) (-10.7639320225002)
15.07.2019|19:06:35.558|[20]|ERROR|TcApplication.MainApp|'X' (Axis-ID: 4, Ctrl-ID: 4): The following error 5.354000 exceeds the permitted limit (5.000000) (error-code: #0x4550) !
15.07.2019|19:06:35.568|[20]|ERROR|TcApplication.MainApp|Event (201), source (799) not found! (17056) (Group/axis consequential error) (Consequential error resulting from another causative error related to another axis within the group. Group/axis consequential errors can occur in relation to master/slave couplings or with multiple axis interpolating DXD groups. If, for instance, it is detected that the following error limit of a master axis has been exceeded, then this consequential error is assigned to all the other master axes and slave axes in this group.) (6) (-10.7639320225002)
15.07.2019|19:07:06.990|[20]|ERROR|TcApplication.MainApp|'X' (Axis-ID: 4, Ctrl-ID: 4): The following error 5.361600 exceeds the permitted limit (5.000000) (error-code: #0x4550) !
15.07.2019|19:07:07.001|[20]|ERROR|TcApplication.MainApp|Event (201), source (799) not found! (17056) (Group/axis consequential error) (Consequential error resulting from another causative error related to another axis within the group. Group/axis consequential errors can occur in relation to master/slave couplings or with multiple axis interpolating DXD groups. If, for instance, it is detected that the following error limit of a master axis has been exceeded, then this consequential error is assigned to all the other master axes and slave axes in this group.) (6) (-10.7639320225002)
15.07.2019|19:07:09.532|[20]|ERROR|TcApplication.MainApp|'X' (Axis-ID: 4, Ctrl-ID: 4): The following error 5.385100 exceeds the permitted limit (5.000000) (error-code: #0x4550) !
15.07.2019|19:07:09.542|[20]|ERROR|TcApplication.MainApp|Event (201), source (799) not found! (17056) (Group/axis consequential error) (Consequential error resulting from another causative error related to another axis within the group. Group/axis consequential errors can occur in relation to master/slave couplings or with multiple axis interpolating DXD groups. If, for instance, it is detected that the following error limit of a master axis has been exceeded, then this consequential error is assigned to all the other master axes and slave axes in this group.) (6) (-10.7639320225002)
15.07.2019|19:07:55.072|[20]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): CoE - Emergency (Hex: %04x, %02x, '%02x %02x %02x %02x %02x').) (Drive 3 (CDHD)) (1002) (61568) (0) (0) (0) (0) (0) (0)
15.07.2019|19:07:55.089|[20]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): CoE - Emergency (Hex: %04x, %02x, '%02x %02x %02x %02x %02x').) (Drive 4 (CDHD)) (1003) (61568) (0) (0) (0) (0) (0) (0)
15.07.2019|19:07:55.120|[20]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): CoE - Emergency (Hex: %04x, %02x, '%02x %02x %02x %02x %02x').) (Drive 3 (CDHD)) (1002) (61568) (0) (0) (0) (0) (0) (0)
15.07.2019|19:07:55.137|[20]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): CoE - Emergency (Hex: %04x, %02x, '%02x %02x %02x %02x %02x').) (Drive 4 (CDHD)) (1003) (61568) (0) (0) (0) (0) (0) (0)
15.07.2019|19:07:55.173|[20]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): CoE - Emergency (Hex: %04x, %02x, '%02x %02x %02x %02x %02x').) (Drive 3 (CDHD)) (1002) (61568) (0) (0) (0) (0) (0) (0)
15.07.2019|19:07:55.188|[20]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): CoE - Emergency (Hex: %04x, %02x, '%02x %02x %02x %02x %02x').) (Drive 4 (CDHD)) (1003) (61568) (0) (0) (0) (0) (0) (0)
15.07.2019|19:13:13.888|[28]|ERROR|TcApplication.MainApp|'Group 4' (Grp-ID: 4): A runtime error has occured in the cyclic SAF-task of the 3D-group (error code: 0x4260) !
15.07.2019|19:13:13.893|[28]|ERROR|TcApplication.MainApp|Event (17022), source (500) not found! (X) (4) (7) (16992) (34620163) (0) (63.851600) (-432.229368)
15.07.2019|19:13:13.897|[28]|ERROR|TcApplication.MainApp|Event (17022), source (500) not found! (Y) (5) (5) (16992) (34620163) (0) (-263.516000) (0.365763)
15.07.2019|19:13:13.902|[28]|ERROR|TcApplication.MainApp|Event (1025), source (11500) not found! (2) (C:\TwinCAT\CNC\DrawOnFly_NCI.NC)
15.07.2019|19:13:13.907|[28]|ERROR|TcApplication.MainApp|Event (201), source (799) not found! (16992) (Controller enable) (Controller enable for the axis or for a coupled slave axis is not present (see axis interface PlcToNc). This error occurs if the controller enable is withdrawn while an axis or a group of axes (also a master/slave group) is being actively positioned. The error also occurs if a PTP axis or a coupled slave axis is started without controller enable.) (1) (59.0472581791172)
15.07.2019|19:13:13.951|[28]|ERROR|TcApplication.MainApp|Event (200), source (703) not found! (16992) (Controller enable) (Controller enable for the axis or for a coupled slave axis is not present (see axis interface PlcToNc). This error occurs if the controller enable is withdrawn while an axis or a group of axes (also a master/slave group) is being actively positioned. The error also occurs if a PTP axis or a coupled slave axis is started without controller enable.) (2) (C:\TwinCAT\CNC\DrawOnFly_NCI.NC) (73) () (NC-Server: v3.1 (Build 4430))
15.07.2019|19:20:12.297|[1]|INFO |TcApplication.MainApp|Application stopped.
17.07.2019|11:30:45.202|[1]|INFO |TcApplication.MainApp|Application started.
17.07.2019|11:30:45.524|[1]|INFO |TcApplication.MainApp|Settings loaded: F:\1 BF资料\11  解决方案\圆盘跟随写LOGO20190717\TC3NCI-STRUCT\TC3NCI_3Axis\NCI_HMI\System\AppSet.xml
17.07.2019|11:30:49.451|[1]|INFO |TcApplication.MainApp|User logged on -> Admin account
17.07.2019|11:31:23.734|[1]|INFO |TcApplication.MainApp|Application stopped.
17.07.2019|11:31:29.847|[1]|INFO |TcApplication.MainApp|Application started.
17.07.2019|11:31:30.148|[1]|INFO |TcApplication.MainApp|Settings loaded: F:\1 BF资料\11  解决方案\圆盘跟随写LOGO20190717\TC3NCI-STRUCT\TC3NCI_3Axis\NCI_HMI\System\AppSet.xml
17.07.2019|11:31:38.873|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Axis Parameter1' PlcVar '.PLCMParList1'
17.07.2019|11:31:38.954|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Axis Parameter2' PlcVar '.PLCMParList2'
17.07.2019|11:31:38.957|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste 3' PlcVar '.PLCMParList3'
17.07.2019|11:31:38.960|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Timer' PlcVar '.PlcMParTimer'
17.07.2019|11:31:38.963|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste Bool' PlcVar '.PLCMParBool'
17.07.2019|11:31:38.966|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste Int' PlcVar '.PLCMParInt'
17.07.2019|11:31:38.969|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Strings' PlcVar '.PLCMParListString'
17.07.2019|11:31:38.986|[1]|INFO |TcApplication.MainApp|User logged on -> Admin account
17.07.2019|11:35:05.306|[11]|ERROR|TcApplication.MainApp|'Y' (Axis-ID: 5, Ctrl-ID: 5): The following error -5.761000 exceeds the permitted limit (5.000000) (error-code: #0x4550) !
17.07.2019|11:41:29.988|[11]|ERROR|TcApplication.MainApp|'Y' (Axis-ID: 5, Ctrl-ID: 5): The following error -5.748000 exceeds the permitted limit (5.000000) (error-code: #0x4550) !
17.07.2019|11:46:54.874|[11]|ERROR|TcApplication.MainApp|'Y' (Axis-ID: 5, Ctrl-ID: 5): The following error -5.749000 exceeds the permitted limit (5.000000) (error-code: #0x4550) !
17.07.2019|11:52:10.186|[11]|ERROR|TcApplication.MainApp|'Y' (Axis-ID: 5, Ctrl-ID: 5): The following error -5.727000 exceeds the permitted limit (5.000000) (error-code: #0x4550) !
17.07.2019|11:54:52.500|[11]|ERROR|TcApplication.MainApp|Event (17938), source (500) not found! (R) (3) (3) (3) ('WcState': working counter error) (18005)
17.07.2019|11:54:52.512|[11]|ERROR|TcApplication.MainApp|Event (17938), source (500) not found! (X) (4) (4) (3) ('WcState': working counter error) (18005)
17.07.2019|11:54:52.524|[11]|ERROR|TcApplication.MainApp|Event (17938), source (500) not found! (Y) (5) (5) (3) ('WcState': working counter error) (18005)
17.07.2019|13:40:04.412|[1]|INFO |TcApplication.MainApp|Application started.
17.07.2019|13:40:04.858|[1]|INFO |TcApplication.MainApp|Settings loaded: F:\1 BF资料\11  解决方案\圆盘跟随写LOGO20190717\TC3NCI-STRUCT\TC3NCI_3Axis\NCI_HMI\System\AppSet.xml
17.07.2019|13:40:14.533|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Axis Parameter1' PlcVar '.PLCMParList1'
17.07.2019|13:40:14.623|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Axis Parameter2' PlcVar '.PLCMParList2'
17.07.2019|13:40:14.634|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste 3' PlcVar '.PLCMParList3'
17.07.2019|13:40:14.636|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Timer' PlcVar '.PlcMParTimer'
17.07.2019|13:40:14.638|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste Bool' PlcVar '.PLCMParBool'
17.07.2019|13:40:14.640|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste Int' PlcVar '.PLCMParInt'
17.07.2019|13:40:14.642|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Strings' PlcVar '.PLCMParListString'
17.07.2019|13:40:14.655|[1]|INFO |TcApplication.MainApp|User logged on -> Admin account
17.07.2019|13:40:38.990|[1]|ERROR|TcApplication.MainApp|Error in SetPLCVar(), PLC variable 'Global_HMI.PLCSpindleOverride'
TwinCAT.Ads.AdsErrorException: Ads-Error 0x745 : Timeout has elapsed.
   at Beckhoff.Forms.TcAdsPlcClient.ReadSymbol(String plcVariableName)
   at TcApplication.FormCnc.GetPLCVar(String plcVariableName) in D:\work\20160214_chb_TC3NCI\New_HMI\20140507\TcApplication\FormCnc.cs:line 1045
17.07.2019|13:40:46.619|[1]|ERROR|TcApplication.MainApp|Error in SetPLCVar(), PLC variable 'Global_HMI.PLCSpindleOverride'
TwinCAT.Ads.AdsErrorException: Ads-Error 0x745 : Timeout has elapsed.
   at Beckhoff.Forms.TcAdsPlcClient.ReadSymbol(String plcVariableName)
   at TcApplication.FormCnc.GetPLCVar(String plcVariableName) in D:\work\20160214_chb_TC3NCI\New_HMI\20140507\TcApplication\FormCnc.cs:line 1045
17.07.2019|13:40:52.121|[1]|ERROR|TcApplication.MainApp|Error in SetPLCVar(), PLC variable 'Global_HMI.PlcAxisEnable'
TwinCAT.Ads.AdsErrorException: Ads-Error 0x745 : Timeout has elapsed.
   at Beckhoff.Forms.TcAdsPlcClient.ReadSymbol(String plcVariableName)
   at TcApplication.FormCnc.GetPLCVar(String plcVariableName) in D:\work\20160214_chb_TC3NCI\New_HMI\20140507\TcApplication\FormCnc.cs:line 1045
17.07.2019|13:40:52.122|[1]|ERROR|TcApplication.MainApp|Error in FormCnc RestoreFunctionStatus()
System.InvalidCastException: Specified cast is not valid.
   at TcApplication.FormCnc.RestoreFunctionStatus(Boolean alwaysUpdate) in D:\work\20160214_chb_TC3NCI\New_HMI\20140507\TcApplication\FormCnc.cs:line 1125
17.07.2019|13:41:47.727|[1]|ERROR|TcApplication.MainApp|Error in SetPLCVar(), PLC variable 'Global_HMI.PLCSpindleOverride'
TwinCAT.Ads.AdsErrorException: Ads-Error 0x745 : Timeout has elapsed.
   at Beckhoff.Forms.TcAdsPlcClient.ReadSymbol(String plcVariableName)
   at TcApplication.FormCnc.GetPLCVar(String plcVariableName) in D:\work\20160214_chb_TC3NCI\New_HMI\20140507\TcApplication\FormCnc.cs:line 1045
17.07.2019|13:42:00.924|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Axis Parameter1' PlcVar '.PLCMParList1'
17.07.2019|13:42:00.933|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Axis Parameter2' PlcVar '.PLCMParList2'
17.07.2019|13:42:00.938|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste 3' PlcVar '.PLCMParList3'
17.07.2019|13:42:00.944|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Timer' PlcVar '.PlcMParTimer'
17.07.2019|13:42:01.010|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste Bool' PlcVar '.PLCMParBool'
17.07.2019|13:42:01.079|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste Int' PlcVar '.PLCMParInt'
17.07.2019|13:42:01.151|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Strings' PlcVar '.PLCMParListString'
17.07.2019|13:42:11.850|[1]|ERROR|TcApplication.MainApp|Module 'Beckhoff.Forms.Nc.TcAdsNcClient' - Internal error in ReadIpolRules_ZeroOffsets_Rot: Ads-Error 0x745 : Timeout has elapsed.
17.07.2019|13:42:16.893|[1]|ERROR|TcApplication.MainApp|Error in SetPLCVar(), PLC variable 'Global_HMI.PLCSpindleOverride'
TwinCAT.Ads.AdsErrorException: Ads-Error 0x745 : Timeout has elapsed.
   at Beckhoff.Forms.TcAdsPlcClient.ReadSymbol(String plcVariableName)
   at TcApplication.FormCnc.GetPLCVar(String plcVariableName) in D:\work\20160214_chb_TC3NCI\New_HMI\20140507\TcApplication\FormCnc.cs:line 1045
17.07.2019|13:42:21.902|[1]|ERROR|TcApplication.MainApp|Error in SetPLCVar(), PLC variable 'Global_HMI.PlcAxisEnable'
TwinCAT.Ads.AdsErrorException: Ads-Error 0x745 : Timeout has elapsed.
   at Beckhoff.Forms.TcAdsPlcClient.ReadSymbol(String plcVariableName)
   at TcApplication.FormCnc.GetPLCVar(String plcVariableName) in D:\work\20160214_chb_TC3NCI\New_HMI\20140507\TcApplication\FormCnc.cs:line 1045
17.07.2019|13:42:47.907|[1]|ERROR|TcApplication.MainApp|Module 'Beckhoff.Forms.Nc.TcAdsNcClient' - Internal error in ReadIpolRules_ZeroOffsets_Rot: Ads-Error 0x745 : Timeout has elapsed.
17.07.2019|13:42:52.912|[1]|ERROR|TcApplication.MainApp|Module 'Beckhoff.Forms.Nc.TcAdsNcClient' - Internal error in ReadIpolRules_ZeroOffsets_Rot: Ads-Error 0x745 : Timeout has elapsed.
17.07.2019|13:54:21.224|[1]|INFO |TcApplication.MainApp|Application started.
17.07.2019|13:54:21.625|[1]|INFO |TcApplication.MainApp|Settings loaded: F:\1 BF资料\11  解决方案\圆盘跟随写LOGO20190717\TC3NCI-STRUCT\TC3NCI_3Axis\NCI_HMI\System\AppSet.xml
17.07.2019|13:54:26.390|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Axis Parameter1' PlcVar '.PLCMParList1'
17.07.2019|13:54:26.480|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Axis Parameter2' PlcVar '.PLCMParList2'
17.07.2019|13:54:26.483|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste 3' PlcVar '.PLCMParList3'
17.07.2019|13:54:26.487|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Timer' PlcVar '.PlcMParTimer'
17.07.2019|13:54:26.499|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste Bool' PlcVar '.PLCMParBool'
17.07.2019|13:54:26.503|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste Int' PlcVar '.PLCMParInt'
17.07.2019|13:54:26.507|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Strings' PlcVar '.PLCMParListString'
17.07.2019|13:54:26.519|[1]|INFO |TcApplication.MainApp|User logged on -> Admin account
17.07.2019|13:55:41.682|[11]|ERROR|TcApplication.MainApp|'X' (Axis-ID: 4): Motion commands are not allowed for external setpoint generated axis (protected mode, check the axis parameter 'allow motion commands to external setpoint axis')(CmdType: 1, Error: 0x4257)
17.07.2019|13:55:41.741|[11]|ERROR|TcApplication.MainApp|'X' (Axis-ID: 4, Grp-ID: 7): Group function is rejected with error-code 0x4257 or the function is not supported !
17.07.2019|13:55:41.750|[11]|ERROR|TcApplication.MainApp|'Y' (Axis-ID: 5): Motion commands are not allowed for external setpoint generated axis (protected mode, check the axis parameter 'allow motion commands to external setpoint axis')(CmdType: 1, Error: 0x4257)
17.07.2019|13:55:41.759|[11]|ERROR|TcApplication.MainApp|'Y' (Axis-ID: 5, Grp-ID: 5): Group function is rejected with error-code 0x4257 or the function is not supported !
17.07.2019|13:58:49.803|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Axis Parameter1' PlcVar '.PLCMParList1'
17.07.2019|13:58:49.807|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Axis Parameter2' PlcVar '.PLCMParList2'
17.07.2019|13:58:49.809|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste 3' PlcVar '.PLCMParList3'
17.07.2019|13:58:49.811|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Timer' PlcVar '.PlcMParTimer'
17.07.2019|13:58:49.813|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste Bool' PlcVar '.PLCMParBool'
17.07.2019|13:58:49.815|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste Int' PlcVar '.PLCMParInt'
17.07.2019|13:58:49.817|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Strings' PlcVar '.PLCMParListString'
17.07.2019|13:59:07.294|[11]|ERROR|TcApplication.MainApp|Event (17022), source (500) not found! (X) (4) (7) (16992) (34608387) (1) (-192.983300) (-38.506772)
17.07.2019|13:59:07.303|[11]|ERROR|TcApplication.MainApp|Event (17022), source (500) not found! (Y) (5) (5) (16992) (34608387) (0) (-192.900000) (-39.107013)
17.07.2019|13:59:27.535|[1]|ERROR|TcApplication.MainApp|Module 'Beckhoff.Forms.Nc.TcAdsNcClient' - Internal error in ReadIpolRules_ZeroOffsets_Rot: Ads-Error 0x745 : Timeout has elapsed.
17.07.2019|13:59:27.598|[1]|ERROR|TcApplication.MainApp|Module 'Beckhoff.Forms.Nc.TcAdsNcClient' - Internal error in ReadIpolRules_ZeroOffsets_Rot: Ads-Error 0x6 : Target port could not be found.
17.07.2019|13:59:43.353|[1]|INFO |TcApplication.MainApp|Application stopped.
17.07.2019|14:00:49.131|[1]|INFO |TcApplication.MainApp|Application started.
17.07.2019|14:00:49.463|[1]|INFO |TcApplication.MainApp|Settings loaded: F:\1 BF资料\11  解决方案\圆盘跟随写LOGO20190717\TC3NCI-STRUCT\TC3NCI_3Axis\NCI_HMI\System\AppSet.xml
17.07.2019|14:00:53.589|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Axis Parameter1' PlcVar '.PLCMParList1'
17.07.2019|14:00:53.672|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Axis Parameter2' PlcVar '.PLCMParList2'
17.07.2019|14:00:53.676|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste 3' PlcVar '.PLCMParList3'
17.07.2019|14:00:53.680|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Timer' PlcVar '.PlcMParTimer'
17.07.2019|14:00:53.684|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste Bool' PlcVar '.PLCMParBool'
17.07.2019|14:00:53.688|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste Int' PlcVar '.PLCMParInt'
17.07.2019|14:00:53.699|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Strings' PlcVar '.PLCMParListString'
17.07.2019|14:00:53.708|[1]|INFO |TcApplication.MainApp|User logged on -> Admin account
17.07.2019|14:03:10.374|[11]|ERROR|TcApplication.MainApp|'X' (Axis-ID: 4, Ctrl-ID: 4): The following error 5.361900 exceeds the permitted limit (5.000000) (error-code: #0x4550) !
17.07.2019|14:03:32.235|[11]|ERROR|TcApplication.MainApp|'X' (Axis-ID: 4, Ctrl-ID: 4): The following error 5.370900 exceeds the permitted limit (5.000000) (error-code: #0x4550) !
17.07.2019|14:14:45.818|[11]|ERROR|TcApplication.MainApp|Event (17022), source (500) not found! (X) (4) (7) (16992) (34620163) (1) (-191.819400) (0.000004)
17.07.2019|14:14:45.827|[11]|ERROR|TcApplication.MainApp|Event (17022), source (500) not found! (Y) (5) (5) (16992) (34620163) (0) (13.182000) (0.000000)
17.07.2019|14:16:57.300|[11]|ERROR|TcApplication.MainApp|Event (17022), source (500) not found! (X) (4) (7) (16992) (34620163) (1) (-188.853300) (0.000209)
17.07.2019|14:16:57.309|[11]|ERROR|TcApplication.MainApp|Event (17022), source (500) not found! (Y) (5) (5) (16992) (34620163) (0) (20.444000) (-0.066627)
17.07.2019|14:19:27.323|[11]|ERROR|TcApplication.MainApp|'Y' (Axis-ID: 5, Ctrl-ID: 5): The following error -5.753000 exceeds the permitted limit (5.000000) (error-code: #0x4550) !
17.07.2019|14:22:23.856|[11]|ERROR|TcApplication.MainApp|'Y' (Axis-ID: 5, Ctrl-ID: 5): The following error -5.756000 exceeds the permitted limit (5.000000) (error-code: #0x4550) !
17.07.2019|14:23:10.151|[1]|ERROR|TcApplication.MainApp|Module 'Beckhoff.Forms.Nc.TcAdsNcClient' - Internal error in ReadIpolRules_ZeroOffsets_Rot: Ads-Error 0x6 : Target port could not be found.
17.07.2019|14:23:46.381|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Axis Parameter1' PlcVar '.PLCMParList1'
17.07.2019|14:23:46.405|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Axis Parameter2' PlcVar '.PLCMParList2'
17.07.2019|14:23:46.407|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste 3' PlcVar '.PLCMParList3'
17.07.2019|14:23:46.409|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Timer' PlcVar '.PlcMParTimer'
17.07.2019|14:23:46.411|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste Bool' PlcVar '.PLCMParBool'
17.07.2019|14:23:46.413|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste Int' PlcVar '.PLCMParInt'
17.07.2019|14:23:46.415|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Strings' PlcVar '.PLCMParListString'
17.07.2019|14:25:59.827|[11]|ERROR|TcApplication.MainApp|'Y' (Axis-ID: 5, Ctrl-ID: 5): The following error -5.764000 exceeds the permitted limit (5.000000) (error-code: #0x4550) !
17.07.2019|14:27:01.807|[11]|ERROR|TcApplication.MainApp|'Y' (Axis-ID: 5, Ctrl-ID: 5): The following error -5.746000 exceeds the permitted limit (5.000000) (error-code: #0x4550) !
17.07.2019|14:27:30.406|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Axis Parameter1' PlcVar '.PLCMParList1'
17.07.2019|14:27:30.409|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Axis Parameter2' PlcVar '.PLCMParList2'
17.07.2019|14:27:30.412|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste 3' PlcVar '.PLCMParList3'
17.07.2019|14:27:30.415|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Timer' PlcVar '.PlcMParTimer'
17.07.2019|14:27:30.418|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste Bool' PlcVar '.PLCMParBool'
17.07.2019|14:27:30.421|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste Int' PlcVar '.PLCMParInt'
17.07.2019|14:27:30.424|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Strings' PlcVar '.PLCMParListString'
17.07.2019|14:28:46.845|[11]|ERROR|TcApplication.MainApp|Event (17938), source (500) not found! (R) (3) (3) (3) ('WcState': working counter error) (18005)
17.07.2019|14:28:46.856|[11]|ERROR|TcApplication.MainApp|Event (17938), source (500) not found! (X) (4) (4) (3) ('WcState': working counter error) (18005)
17.07.2019|14:28:46.869|[11]|ERROR|TcApplication.MainApp|Event (17938), source (500) not found! (Y) (5) (5) (3) ('WcState': working counter error) (18005)
17.07.2019|14:29:55.356|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): CoE - Emergency (Hex: %04x, %02x, '%02x %02x %02x %02x %02x').) (Drive 3 (CDHD)) (1002) (28802) (0) (0) (0) (0) (0) (0)
17.07.2019|14:29:55.365|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): CoE - Emergency (Hex: %04x, %02x, '%02x %02x %02x %02x %02x').) (Drive 3 (CDHD)) (1002) (28802) (0) (0) (0) (0) (0) (0)
17.07.2019|14:29:55.374|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): CoE - Emergency (Hex: %04x, %02x, '%02x %02x %02x %02x %02x').) (Drive 3 (CDHD)) (1002) (28802) (0) (0) (0) (0) (0) (0)
17.07.2019|14:30:08.087|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): CoE - Emergency (Hex: %04x, %02x, '%02x %02x %02x %02x %02x').) (Drive 3 (CDHD)) (1002) (28802) (0) (0) (0) (0) (0) (0)
17.07.2019|14:30:08.096|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): CoE - Emergency (Hex: %04x, %02x, '%02x %02x %02x %02x %02x').) (Drive 3 (CDHD)) (1002) (28802) (0) (0) (0) (0) (0) (0)
17.07.2019|14:30:08.105|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): CoE - Emergency (Hex: %04x, %02x, '%02x %02x %02x %02x %02x').) (Drive 3 (CDHD)) (1002) (28802) (0) (0) (0) (0) (0) (0)
17.07.2019|14:32:43.266|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Axis Parameter1' PlcVar '.PLCMParList1'
17.07.2019|14:32:43.268|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Axis Parameter2' PlcVar '.PLCMParList2'
17.07.2019|14:32:43.270|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste 3' PlcVar '.PLCMParList3'
17.07.2019|14:32:43.272|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Timer' PlcVar '.PlcMParTimer'
17.07.2019|14:32:43.274|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste Bool' PlcVar '.PLCMParBool'
17.07.2019|14:32:43.276|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste Int' PlcVar '.PLCMParInt'
17.07.2019|14:32:43.278|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Strings' PlcVar '.PLCMParListString'
17.07.2019|14:32:51.112|[11]|ERROR|TcApplication.MainApp|Event (17938), source (500) not found! (R) (3) (3) (122) ('WcState': working counter error) (18005)
17.07.2019|14:32:51.123|[11]|ERROR|TcApplication.MainApp|Event (17938), source (500) not found! (X) (4) (4) (122) ('WcState': working counter error) (18005)
17.07.2019|14:32:51.135|[11]|ERROR|TcApplication.MainApp|Event (17938), source (500) not found! (Y) (5) (5) (122) ('WcState': working counter error) (18005)
17.07.2019|14:34:42.464|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): CoE - Emergency (Hex: %04x, %02x, '%02x %02x %02x %02x %02x').) (Drive 4 (CDHD)) (1003) (30080) (0) (0) (0) (0) (0) (0)
17.07.2019|14:34:49.266|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): Timeout: '%s'.) (Drive 3 (CDHD)) (1002) (clear sm pdos (0x1C12))
17.07.2019|14:34:49.275|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): state change aborted (requested '%s', back to '%s').) (Drive 3 (CDHD)) (1002) (OP) (PREOP)
17.07.2019|14:34:49.285|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): Timeout: '%s'.) (Drive 4 (CDHD)) (1003) (clear sm pdos (0x1C12))
17.07.2019|14:34:49.293|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): state change aborted (requested '%s', back to '%s').) (Drive 4 (CDHD)) (1003) (OP) (PREOP)
17.07.2019|14:36:16.428|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): Timeout: '%s'.) (Drive 3 (CDHD)) (1002) (clear sm pdos (0x1C12))
17.07.2019|14:36:16.440|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): state change aborted (requested '%s', back to '%s').) (Drive 3 (CDHD)) (1002) (SAFEOP) (PREOP)
17.07.2019|14:37:18.484|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): Timeout: '%s'.) (Drive 3 (CDHD)) (1002) (clear sm pdos (0x1C12))
17.07.2019|14:37:18.496|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): state change aborted (requested '%s', back to '%s').) (Drive 3 (CDHD)) (1002) (SAFEOP) (PREOP)
17.07.2019|14:39:54.589|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Axis Parameter1' PlcVar '.PLCMParList1'
17.07.2019|14:39:54.592|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Axis Parameter2' PlcVar '.PLCMParList2'
17.07.2019|14:39:54.595|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste 3' PlcVar '.PLCMParList3'
17.07.2019|14:39:54.598|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Timer' PlcVar '.PlcMParTimer'
17.07.2019|14:39:54.601|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste Bool' PlcVar '.PLCMParBool'
17.07.2019|14:39:54.604|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste Int' PlcVar '.PLCMParInt'
17.07.2019|14:39:54.607|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Strings' PlcVar '.PLCMParListString'
17.07.2019|14:41:35.684|[1]|ERROR|TcApplication.MainApp|Error in FKeyWriteSymbol()
TwinCAT.Ads.AdsDatatypeNotSupportedException: Symbol not found. PLC variable: .PLCStoerungLoeschen
   at Beckhoff.Forms.TcAdsPlcClient.WriteSymbol(String plcVariableName, String valueString)
   at TcApplication.FormCnc.FKeyWriteSymbol(String symbol, String value) in D:\work\20160214_chb_TC3NCI\New_HMI\20140507\TcApplication\FormCnc.cs:line 352
17.07.2019|14:43:06.399|[11]|ERROR|TcApplication.MainApp|'Y' (Axis-ID: 5, Ctrl-ID: 5): The following error -5.749000 exceeds the permitted limit (5.000000) (error-code: #0x4550) !
17.07.2019|14:46:20.080|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): abnormal state change (from '%s' to '%s') with code 0x%x, '%s'. Try to go back to '%s'...) (Drive 4 (CDHD)) (1003) (OP) (PREOP) (50) (DC PLL sync error) (OP)
17.07.2019|14:46:25.113|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): Timeout: '%s'.) (Drive 4 (CDHD)) (1003) (clear sm pdos (0x1C12))
17.07.2019|14:46:25.122|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): state change aborted (requested '%s', back to '%s').) (Drive 4 (CDHD)) (1003) (OP) (PREOP)
17.07.2019|14:50:50.847|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): abnormal state change (from '%s' to '%s') with code 0x%x, '%s'. Try to go back to '%s'...) (Drive 3 (CDHD)) (1002) (OP) (PREOP) (50) (DC PLL sync error) (OP)
17.07.2019|14:50:55.870|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): Timeout: '%s'.) (Drive 3 (CDHD)) (1002) (clear sm pdos (0x1C12))
17.07.2019|14:50:55.879|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): state change aborted (requested '%s', back to '%s').) (Drive 3 (CDHD)) (1002) (OP) (PREOP)
17.07.2019|14:53:03.028|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): abnormal state change (from '%s' to '%s') with code 0x%x, '%s'. Try to go back to '%s'...) (Drive 1 (CDHD)) (1001) (OP) (PREOP) (50) (DC PLL sync error) (OP)
17.07.2019|14:53:08.054|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): Timeout: '%s'.) (Drive 1 (CDHD)) (1001) (clear sm pdos (0x1C12))
17.07.2019|14:53:08.066|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): state change aborted (requested '%s', back to '%s').) (Drive 1 (CDHD)) (1001) (OP) (PREOP)
17.07.2019|14:53:27.517|[1]|ERROR|TcApplication.MainApp|Module 'Beckhoff.Forms.Nc.TcAdsNcClient' - Internal error in ReadIpolRules_ZeroOffsets_Rot: Ads-Error 0x6 : Target port could not be found.
17.07.2019|14:53:36.009|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): Timeout: '%s'.) (Drive 1 (CDHD)) (1001) (clear sm pdos (0x1C12))
17.07.2019|14:53:36.020|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): state change aborted (requested '%s', back to '%s').) (Drive 1 (CDHD)) (1001) (SAFEOP) (PREOP)
17.07.2019|14:53:36.031|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): Timeout: '%s'.) (Drive 3 (CDHD)) (1002) (clear sm pdos (0x1C12))
17.07.2019|14:53:36.043|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): state change aborted (requested '%s', back to '%s').) (Drive 3 (CDHD)) (1002) (SAFEOP) (PREOP)
17.07.2019|14:53:36.055|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): Timeout: '%s'.) (Drive 4 (CDHD)) (1003) (clear sm pdos (0x1C12))
17.07.2019|14:53:36.067|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): state change aborted (requested '%s', back to '%s').) (Drive 4 (CDHD)) (1003) (SAFEOP) (PREOP)
17.07.2019|14:54:06.335|[1]|ERROR|TcApplication.MainApp|Module 'Beckhoff.Forms.Nc.TcAdsNcClient' - Internal error in ReadChannelCyclic:
Group: 0x2102
Offset: 0x12
Ads-Error 0x6 : Target port could not be found.
17.07.2019|14:54:06.346|[1]|ERROR|TcApplication.MainApp|Module 'Beckhoff.Forms.Nc.TcAdsNcClient' - Internal error in ReadIpolRules_ZeroOffsets_Rot: Ads-Error 0x6 : Target port could not be found.
17.07.2019|14:54:14.557|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): Timeout: '%s'.) (Drive 1 (CDHD)) (1001) (clear sm pdos (0x1C12))
17.07.2019|14:54:14.569|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): state change aborted (requested '%s', back to '%s').) (Drive 1 (CDHD)) (1001) (SAFEOP) (PREOP)
17.07.2019|14:54:14.581|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): Timeout: '%s'.) (Drive 3 (CDHD)) (1002) (clear sm pdos (0x1C12))
17.07.2019|14:54:14.593|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): state change aborted (requested '%s', back to '%s').) (Drive 3 (CDHD)) (1002) (SAFEOP) (PREOP)
17.07.2019|14:54:14.605|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): Timeout: '%s'.) (Drive 4 (CDHD)) (1003) (clear sm pdos (0x1C12))
17.07.2019|14:54:14.617|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): state change aborted (requested '%s', back to '%s').) (Drive 4 (CDHD)) (1003) (SAFEOP) (PREOP)
17.07.2019|14:54:53.528|[1]|ERROR|TcApplication.MainApp|Module 'Beckhoff.Forms.Nc.TcAdsNcClient' - Internal error in ReadIpolRules_ZeroOffsets_Rot: Ads-Error 0x6 : Target port could not be found.
17.07.2019|14:55:28.543|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Axis Parameter1' PlcVar '.PLCMParList1'
17.07.2019|14:55:28.545|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Axis Parameter2' PlcVar '.PLCMParList2'
17.07.2019|14:55:28.547|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste 3' PlcVar '.PLCMParList3'
17.07.2019|14:55:28.549|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Timer' PlcVar '.PlcMParTimer'
17.07.2019|14:55:28.551|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste Bool' PlcVar '.PLCMParBool'
17.07.2019|14:55:28.553|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste Int' PlcVar '.PLCMParInt'
17.07.2019|14:55:28.555|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Strings' PlcVar '.PLCMParListString'
17.07.2019|15:00:59.021|[11]|ERROR|TcApplication.MainApp|'Y' (Axis-ID: 5, Ctrl-ID: 5): The following error -5.748000 exceeds the permitted limit (5.000000) (error-code: #0x4550) !
17.07.2019|15:01:39.507|[11]|ERROR|TcApplication.MainApp|Event (17938), source (500) not found! (R) (3) (3) (3) ('WcState': working counter error) (18005)
17.07.2019|15:01:39.519|[11]|ERROR|TcApplication.MainApp|Event (17938), source (500) not found! (X) (4) (4) (3) ('WcState': working counter error) (18005)
17.07.2019|15:01:39.531|[11]|ERROR|TcApplication.MainApp|Event (17938), source (500) not found! (Y) (5) (5) (3) ('WcState': working counter error) (18005)
17.07.2019|15:07:25.235|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): Timeout: '%s'.) (Drive 1 (CDHD)) (1001) (clear sm pdos (0x1C12))
17.07.2019|15:07:25.244|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): state change aborted (requested '%s', back to '%s').) (Drive 1 (CDHD)) (1001) (SAFEOP) (PREOP)
17.07.2019|15:07:25.253|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): Timeout: '%s'.) (Drive 3 (CDHD)) (1002) (clear sm pdos (0x1C12))
17.07.2019|15:07:25.262|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): state change aborted (requested '%s', back to '%s').) (Drive 3 (CDHD)) (1002) (SAFEOP) (PREOP)
17.07.2019|15:07:25.270|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): Timeout: '%s'.) (Drive 4 (CDHD)) (1003) (clear sm pdos (0x1C12))
17.07.2019|15:07:25.280|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): state change aborted (requested '%s', back to '%s').) (Drive 4 (CDHD)) (1003) (SAFEOP) (PREOP)
17.07.2019|15:07:41.182|[1]|ERROR|TcApplication.MainApp|Module 'Beckhoff.Forms.Nc.TcAdsNcClient' - Internal error in ReadIpolRules_ZeroOffsets_Rot: Ads-Error 0x6 : Target port could not be found.
17.07.2019|15:08:06.549|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): Timeout: '%s'.) (Drive 1 (CDHD)) (1001) (clear sm pdos (0x1C12))
17.07.2019|15:08:06.561|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): state change aborted (requested '%s', back to '%s').) (Drive 1 (CDHD)) (1001) (SAFEOP) (PREOP)
17.07.2019|15:08:06.573|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): Timeout: '%s'.) (Drive 3 (CDHD)) (1002) (clear sm pdos (0x1C12))
17.07.2019|15:08:06.585|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): state change aborted (requested '%s', back to '%s').) (Drive 3 (CDHD)) (1002) (SAFEOP) (PREOP)
17.07.2019|15:08:06.597|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): Timeout: '%s'.) (Drive 4 (CDHD)) (1003) (clear sm pdos (0x1C12))
17.07.2019|15:08:06.609|[11]|ERROR|TcApplication.MainApp|Event (1), source (10) not found! ('%s' (%d): state change aborted (requested '%s', back to '%s').) (Drive 4 (CDHD)) (1003) (SAFEOP) (PREOP)
17.07.2019|15:08:22.452|[1]|ERROR|TcApplication.MainApp|Module 'Beckhoff.Forms.Nc.TcAdsNcClient' - Internal error in ReadIpolRules_ZeroOffsets_Rot: Ads-Error 0x6 : Target port could not be found.
17.07.2019|15:08:22.461|[1]|ERROR|TcApplication.MainApp|Module 'Beckhoff.Forms.Nc.TcAdsNcClient' - Internal error in ReadIpolRules_ZeroOffsets_Rot: Ads-Error 0x6 : Target port could not be found.
17.07.2019|15:08:22.472|[1]|ERROR|TcApplication.MainApp|Module 'Beckhoff.Forms.Nc.TcAdsNcClient' - Internal error in ReadIpolRules_ZeroOffsets_Rot: Ads-Error 0x6 : Target port could not be found.
17.07.2019|15:08:22.480|[1]|ERROR|TcApplication.MainApp|Module 'Beckhoff.Forms.Nc.TcAdsNcClient' - Internal error in ReadIpolRules_ZeroOffsets_Rot: Ads-Error 0x6 : Target port could not be found.
17.07.2019|15:08:22.488|[1]|ERROR|TcApplication.MainApp|Module 'Beckhoff.Forms.Nc.TcAdsNcClient' - Internal error in ReadIpolRules_ZeroOffsets_Rot: Ads-Error 0x6 : Target port could not be found.
17.07.2019|15:08:22.496|[1]|ERROR|TcApplication.MainApp|Module 'Beckhoff.Forms.Nc.TcAdsNcClient' - Internal error in ReadIpolRules_ZeroOffsets_Rot: Ads-Error 0x6 : Target port could not be found.
17.07.2019|15:08:22.504|[1]|ERROR|TcApplication.MainApp|Module 'Beckhoff.Forms.Nc.TcAdsNcClient' - Internal error in ReadIpolRules_ZeroOffsets_Rot: Ads-Error 0x6 : Target port could not be found.
17.07.2019|15:08:22.512|[1]|ERROR|TcApplication.MainApp|Module 'Beckhoff.Forms.Nc.TcAdsNcClient' - Internal error in ReadIpolRules_ZeroOffsets_Rot: Ads-Error 0x6 : Target port could not be found.
17.07.2019|15:08:22.520|[1]|ERROR|TcApplication.MainApp|Module 'Beckhoff.Forms.Nc.TcAdsNcClient' - Internal error in ReadIpolRules_ZeroOffsets_Rot: Ads-Error 0x6 : Target port could not be found.
17.07.2019|15:08:22.528|[1]|ERROR|TcApplication.MainApp|Module 'Beckhoff.Forms.Nc.TcAdsNcClient' - Internal error in ReadIpolRules_ZeroOffsets_Rot: Ads-Error 0x6 : Target port could not be found.
17.07.2019|15:08:22.536|[1]|ERROR|TcApplication.MainApp|Module 'Beckhoff.Forms.Nc.TcAdsNcClient' - Internal error in ReadIpolRules_ZeroOffsets_Rot: Ads-Error 0x6 : Target port could not be found.
17.07.2019|15:08:59.080|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Axis Parameter1' PlcVar '.PLCMParList1'
17.07.2019|15:08:59.084|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Axis Parameter2' PlcVar '.PLCMParList2'
17.07.2019|15:08:59.088|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste 3' PlcVar '.PLCMParList3'
17.07.2019|15:08:59.092|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Timer' PlcVar '.PlcMParTimer'
17.07.2019|15:08:59.095|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste Bool' PlcVar '.PLCMParBool'
17.07.2019|15:08:59.099|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste Int' PlcVar '.PLCMParInt'
17.07.2019|15:08:59.103|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Strings' PlcVar '.PLCMParListString'
17.07.2019|15:24:06.115|[1]|ERROR|TcApplication.MainApp|Module 'Beckhoff.Forms.Nc.TcAdsNcClient' - Internal error in ReadChannelCyclic:
Group: 0x2102
Offset: 0x12
Ads-Error 0x745 : Timeout has elapsed.
17.07.2019|15:24:11.127|[1]|ERROR|TcApplication.MainApp|Module 'Beckhoff.Forms.Nc.TcAdsNcClient' - Internal error in ReadChannelCyclic:
Group: 0x2102
Offset: 0x12
Ads-Error 0x745 : Timeout has elapsed.
17.07.2019|15:24:23.566|[1]|ERROR|TcApplication.MainApp|Error in SetPLCVar(), PLC variable 'Global_HMI.PLCSpindleOverride'
TwinCAT.Ads.AdsErrorException: Ads-Error 0x745 : Timeout has elapsed.
   at Beckhoff.Forms.TcAdsPlcClient.ReadSymbol(String plcVariableName)
   at TcApplication.FormCnc.GetPLCVar(String plcVariableName) in D:\work\20160214_chb_TC3NCI\New_HMI\20140507\TcApplication\FormCnc.cs:line 1045
17.07.2019|15:24:33.393|[1]|ERROR|TcApplication.MainApp|Error in SetPLCVar(), PLC variable 'Global_HMI.PLCSpindleOverride'
TwinCAT.Ads.AdsErrorException: Ads-Error 0x745 : Timeout has elapsed.
   at Beckhoff.Forms.TcAdsPlcClient.ReadSymbol(String plcVariableName)
   at TcApplication.FormCnc.GetPLCVar(String plcVariableName) in D:\work\20160214_chb_TC3NCI\New_HMI\20140507\TcApplication\FormCnc.cs:line 1045
17.07.2019|15:25:23.017|[1]|ERROR|TcApplication.MainApp|Module 'Beckhoff.Forms.Nc.TcAdsNcClient' - ReadGroupInfo: TwinCAT.Ads.AdsErrorException: Ads-Error 0x745 : Timeout has elapsed.
   at TwinCAT.Ads.Internal.TcAdsDllWrapper.ThrowAdsException(AdsErrorCode adsErrorCode)
   at TwinCAT.Ads.Internal.TcAdsSyncPortRouter.Read(UInt32 indexGroup, UInt32 indexOffset, Int32 length, Void* data, Boolean throwAdsException, Int32& dataRead)
   at TwinCAT.Ads.Internal.TcAdsDllWrapper.Read(UInt32 indexGroup, UInt32 indexOffset, Int32 offset, Int32 length, Byte[] data, Boolean throwAdsException, Int32& dataRead)
   at TwinCAT.Ads.TcAdsClient.Read(Int32 indexGroup, Int32 indexOffset, AdsStream dataStream, Int32 offset, Int32 length)
   at Beckhoff.Forms.Nc.TcAdsNci.c()
17.07.2019|15:25:32.437|[1]|ERROR|TcApplication.MainApp|Module 'Beckhoff.Forms.Nc.TcAdsNcClient' - Internal error in ReadChannelCyclic:
Group: 0x2102
Offset: 0x12
Ads-Error 0x745 : Timeout has elapsed.
17.07.2019|15:25:37.443|[1]|ERROR|TcApplication.MainApp|Module 'Beckhoff.Forms.Nc.TcAdsNcClient' - Internal error in ReadChannelCyclic:
Group: 0x2102
Offset: 0x12
Ads-Error 0x745 : Timeout has elapsed.
17.07.2019|15:26:35.843|[1]|ERROR|TcApplication.MainApp|Error in SetPLCVar(), PLC variable 'Global_HMI.PLCSpindleOverride'
TwinCAT.Ads.AdsErrorException: Ads-Error 0x745 : Timeout has elapsed.
   at Beckhoff.Forms.TcAdsPlcClient.ReadSymbol(String plcVariableName)
   at TcApplication.FormCnc.GetPLCVar(String plcVariableName) in D:\work\20160214_chb_TC3NCI\New_HMI\20140507\TcApplication\FormCnc.cs:line 1045
17.07.2019|15:33:39.308|[1]|ERROR|TcApplication.MainApp|Module 'Beckhoff.Forms.Nc.TcAdsNcClient' - Internal error in ReadChannelCyclic:
Group: 0x2102
Offset: 0x12
Ads-Error 0x745 : Timeout has elapsed.
17.07.2019|15:33:44.314|[1]|ERROR|TcApplication.MainApp|Module 'Beckhoff.Forms.Nc.TcAdsNcClient' - Internal error in ReadChannelCyclic:
Group: 0x2102
Offset: 0x12
Ads-Error 0x745 : Timeout has elapsed.
17.07.2019|15:33:45.087|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Axis Parameter1' PlcVar '.PLCMParList1'
17.07.2019|15:33:45.097|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Axis Parameter2' PlcVar '.PLCMParList2'
17.07.2019|15:33:45.108|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste 3' PlcVar '.PLCMParList3'
17.07.2019|15:33:45.117|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Timer' PlcVar '.PlcMParTimer'
17.07.2019|15:33:45.127|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste Bool' PlcVar '.PLCMParBool'
17.07.2019|15:33:45.138|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Liste Int' PlcVar '.PLCMParInt'
17.07.2019|15:33:45.148|[1]|ERROR|TcApplication.MainApp|Machine parameter list cannot be written to the Plc! Symbol not found! List 'Strings' PlcVar '.PLCMParListString'
17.07.2019|15:34:06.737|[1]|ERROR|TcApplication.MainApp|Error in SetPLCVar(), PLC variable 'Global_HMI.PLCSpindleOverride'
TwinCAT.Ads.AdsErrorException: Ads-Error 0x745 : Timeout has elapsed.
   at Beckhoff.Forms.TcAdsPlcClient.ReadSymbol(String plcVariableName)
   at TcApplication.FormCnc.GetPLCVar(String plcVariableName) in D:\work\20160214_chb_TC3NCI\New_HMI\20140507\TcApplication\FormCnc.cs:line 1045
